;=============================================================================================================================
;
;  README for GeneralTouch RS232,AcousticdWave Touchscreen driver for Windows 2000/Xp package.
;
;  Version 3.0.0
;
;  PnP_compliant version.
;	
;  Copyright 1998-2002,General Touch Technology Co., Ltd. All rights reserved.
;
;=============================================================================================================================
   
Thank you for choosing our RS232,AcousticWave Touchscreen products!! This README file contains
additional notes about our touchscreen software which,we think,will help you make better use of
our touchscreen and touchscreen software.

==================================
Supported Touchscreen controller
==================================

	- GeneralTouch PnP-compliant serial controller 5041 
	
  	 --------------------------------------------------------
  	|                                                        |
  	|  This driver does not support GeneralTouch serial      |
	|  controller 2036,2037,4001s,4001s-M and usb controller |
  	|  2038,4001U.					         |
  	|                                                        |
  	|  Refer to www.Generaltouch.com for availability of	 | 
	|  drivers for these products.                           |
  	|                                                        |
   	--------------------------------------------------------

=========
CONTENTS
=========
1.Install/Uninstall Manual
  1.1 Install touchscreen software
  1.2 Change touchscreen settings
  1.3 Uninstall touchscreen software
  1.4 Release Notes	
2.Software package component
3.Problem solution
4.Update info
5.Contact GeneralTouch

=====================================
1.	Install/Uninstall Manual
=====================================

1.1	Install touchscreen software
====================================================================================

	NOTES: you must have administrator access rights on your 
	Windows 2000 system to install our touchscreen software package 
	for Windows 2000. You must also have administrator access rights 
	to run the touchscreen control panel and touchscreen calibration 
	applications.

    1. Shutdown Windows and turn off your computer.

    2. Install your touchscreen hardware.

    3. Start your computer.

    4. Windows STARTS the New Hardware Wizard, Choose "Next". 
       Select "Search for the best driver for your device (Recommended)" 
       and Choose "Next".

    5. When a list of search locations is displayed, place a
       checkmark on the floppy drive containing this driver
       for Windows disk. Insert the disk into your floppy drive.
       (If the driver files have been copied to your hard drive or
       have been distributed on CD, place a checkmark on "Specify
       a location" and use Browse to select the directory
       containing the driver files.)

    6. Choose "Next". Once the GeneralTouch Touchscreen serial interface driver
       has been detected choose "Next" again.

    7. Wait while driver files are copied to your computer. Insert
       your Windows CD if prompted.

    8. Choose "Finish", restart your Windows system when prompted. 
       The touchscreen calibration program will automatically run. 
       Touch the three targets as they appear on the screen. 
       Click "Yes" when the cursor lines up correctly with your finger.

======================================================
1.2 	Change Touchscreen settings
======================================================

    1. Click the "Start" button, point to "Settings", and then "control panel".

    2. Double-click the "GeneralTouch Touchscreen" icon, now you can change touchscreen settings.
       for more information about using touchscreen,see context_sensitive help.

======================================================
1.3 	Uninstall Touchscreen software
======================================================

    1. Click the "Start" button, point to "Settings", and then "Control Panel".

    2. Double-click the "System" Programs icon.

    3. Open device manager, get the "GeneralTouch Touchscreen serial interface" device
       from the list of all devices in the system.

    4. Click the "Remove" button then follow the directions on your screen.

    5. Restart Windows to complete the uninstall process.

=======================================================
1.4 	Release Notes
=======================================================

    1. You must have administrator access rights to run the Touchscreen control panel 
       and Touchscreen calibration applications.

    2. Add options to the control panel,calibration program can be adjusted to run every
       time that the computer is rebooted.

======================================
2.	Software Component
======================================

Our touchscreen software package for Windows 2000 is composed of the following programs:

	  GenTouch.Sys	             Our PnP-compliant touchscreen driver.	

          GenPanel.Cpl               32 bit touchscreen control panel.

	  GenCoInst.dll	     32 bit touchscreen device co_installer.

          GenCalib.exe               32 bit touchscreen calibration program.

	  GenHelp.Hlp                Touchscreen help file, you can get more
				     information about our product and device settings.
     
	  GenTouch.Inf		     our touchscreen device install information file
	
          README.txt                 It's me!


====================================
3.	Problem solution
====================================

-  The system mouse class driver MOUCLASS.SYS is required by the driver. most times,
   it is installed during Windows installation process. if not,our device driver 
   will not work.

-  Our device driver depends on the Windows beep service (BEEP.SYS) to make audible 
   feedback,so if beep service (BEEP.SYS) does not work,there will be no beep here.

====================================
4. 	Update info
====================================

-  Calibration program automatically runs when touchscreen device has just installed successfully.

-  Add options to the control panel, calibration program can be adjusted to run every time that computer
   is rebooted.
      
====================================
5.	Contact	GeneralTouch
====================================

General Touch Technology Co., Ltd.

Sunsing High-Tech Zone,
No.8 Shuangxing North Road,
Xiejiaci,Chengdu,Sichuan,P.R.China

Tel:(86)28-87344128
Fax:(86)28-87341133

http://www.generaltouch.com

;=============================================================================================================================
;
;                                      Copyright 1998-2003, General Touch Technology Co., Ltd.
;
;                                                   All rights reserved.
;
;
;=============================================================================================================================

